# Potkrovlje - izolacija krova i koncept uredjenja

Datum provere cena: 2026-03-25

## 1. Sta sam uzeo kao bazu
- Bruto povrsina iz dostavljene tabele: `79.29 m2`
- Povrsina terase iz tabele: `5.89 m2`
- Za krov sam radio dve varijante:
  - ako terasa nije pod krovom: `76.92 m2` kosina
  - ako puna bruto projekcija ulazi u krov: `83.09 m2` kosina
- Za nabavku sam kao realan radni scenario uzeo:
  - `84.61 m2` sa 10% rezerve u varijanti bez terase pod krovom
  - gornji bezbedni scenario: `91.40 m2` sa 10% rezerve

## 2. Moja tehnicka preporuka

### Preporuceni sistem
Od spolja ka unutra:
1. postojeci crep
2. postojeca paropropusna folija
3. postojece daske
4. proverena ventilisana distanca 3-5 cm ako membrana nije sigurno potvrdena kao ispravna i dovoljno difuzno otvorena
5. 10 cm kamena vuna izmedju rogova
6. dodatnih 5 cm ili 10 cm ispod rogova u kontinuitetu
7. unutrasnja aktivna parna brana / pametna membrana ili bar kvalitetna parna brana sa zadihtovanim spojnicama
8. podkonstrukcija za instalacioni sloj
9. drvena obloga - lamperija ili brodski pod, ne gips

### Sta je najpametnije za tvoj slucaj
- Ako hoces balans cena / trajnost / zvuk / protivpozarno: `20 cm ukupno` mineralne vune i drvena obloga.
- Ako hoces da ustedis, ali da i dalje bude korektno: `15 cm ukupno`.
- Ako membrana ispod crepa nije proverena ili je starija i nepoznata, ja ne bih nabijao vunu direktno u daske bez kontrole detalja.

### Ocekivani termicki nivo
- `15 cm` mineralne vune: okvirno `U oko 0.23-0.26 W/m2K`
- `20 cm` mineralne vune: okvirno `U oko 0.18-0.21 W/m2K`

Zakljucak: za potkrovlje koje zelis da koristis kao ozbiljan stambeni prostor, ja bih isao na `20 cm`.

## 3. Kvadratura i kolicine

### Radna nabavna kvadratura
- Preporuka za obracun i porucivanje: `85 m2`
- Ako zelis potpuno bezbednu gornju rezervu: `91-92 m2`

### Zapremina izolacije
- Za `15 cm`: oko `12.69 m3` izolacije sa rezervom
- Za `20 cm`: oko `16.92 m3` izolacije sa rezervom

## 4. Cene sa neta i kako sam ih citao

### Izolacija i membrane
- `NaturBoard FIT Plus Knauf` na Roma: `od 436 RSD/kom`, proizvod za kosi krov, kamena vuna. Na Knauf oficijelnom listu za varijantu 100 mm stoji ploca `600 x 1000 mm`, 6 kom u paketu = `3.60 m2/pak`. Iz toga izlazi maloprodajni reper od oko `727 RSD/m2` za `10 cm`.
- `KNAUF PARNA BRANA LDS 5 Silk 75m2` na Roma: `10,030 RSD/rolna`
- `KNAUF PARNA BRANA LDS 200 AluPlus 75m2` na Roma: `8,685 RSD/rolna`
- `Knauf HomeSeal LDS Solifit 1 25m` na Roma: `2,050 RSD/rolna`

### Drvena podkonstrukcija i obloga
- `Letva 3x5 3m` na Crafter: `259 RSD/kom`
- `Lamperija severna jela` na Krajina drvo / KP: `1,370 RSD/m2`
- `Camova lamperija 10 mm` na Krajina drvo: `1,000 RSD/m2`
- Premium sauna omorika na Aquaplan: `460 RSD/m duzni`, a za `1 m2` treba `10.52 m duznih`, sto izadje oko `4,839 RSD/m2`

### Ruke - reperi sa trzista
- Daibau za izolaciju potkrovlja daje vise stavki po m2; za `NaturBoard FIT PLUS` prikaz je `5.30-7.90 EUR/m2`, a za `Homeseal LDS 0.02` oko `0.80 EUR/m2`
- Svezaskele navodi prosecnu cenu izolacije potkrovlja `7-12 EUR/m2 plus materijal`

### Sta iz ovoga zakljucujem
- Cene materijala za Srbiju koje sam nasao online podrzavaju realan raspon:
  - izolacija `15 cm`: oko `1,100-1,300 RSD/m2`
  - izolacija `20 cm`: oko `1,450-1,700 RSD/m2`
  - kvalitetna unutrasnja membrana: oko `135-200 RSD/m2` po rolnama, ali sa realnim nabavnim otpadom racunaj vise
  - drvena obloga: realno `1,000-1,370 RSD/m2` za normalnu enterijersku lamperiju

## 5. Troskovnik koji bih ja koristio za odluku

Napomena: ovo je `procena`, ne ponuda izvodjaca. U total nisam stavljao teske opravke krova, zamenu trulih dasaka, novu foliju spolja, skelu spolja ili dekorativnu rasvetu.

### Varijanta A - korektna i racionalna, 15 cm
- Obracunska povrsina: `84.61 m2`
- Materijal okvirno: `288,000-311,000 RSD`
- Ruke okvirno: `129,000-179,000 RSD`
- Ukupno okvirno: `418,000-490,000 RSD`

Sta dobijas:
- 10 cm izmedju rogova + 5 cm dodatni sloj
- parna brana / aktivna membrana
- podkonstrukcija
- drvena lamperija kao final

### Varijanta B - moja preporuka, 20 cm
- Obracunska povrsina: `84.61 m2`
- Materijal okvirno: `354,000-378,000 RSD`
- Ruke okvirno: `148,000-208,000 RSD`
- Ukupno okvirno: `502,000-586,000 RSD`

Sta dobijas:
- 20 cm ukupne izolacije
- bolji zimski komfor i bolju zastitu leti
- manji rizik da kasnije pozelis jos jedan dodatni sloj

### Gornji scenario ako se na licu mesta ispostavi da treba racunati punih 91-92 m2
- 15 cm: oko `447,000-524,000 RSD`
- 20 cm: oko `535,000-625,000 RSD`

### Moj savet za budzet
- Ako zelis da uradis jednom i mirno: planiraj `550,000-620,000 RSD` za preporucenu varijantu 20 cm.
- Ako zelis da ne preteras, ali da bude dobro: planiraj `440,000-500,000 RSD` za 15 cm.
- Obe varijante dodatno zastiti sa jos `5-10%` rezerve za nepredvidjene detalje oko terasnih vrata, prodora, stepenisnog otvora i eventualnih krivih rogova.

## 6. Dizajn preporuka za samo potkrovlje

## Glavna ideja koju preporucujem
`Warm Nordic Loft` je najbolja osnova za tvoj prostor jer vec imas:
- lepu opeku na zabatima
- vidljivu drvenu krovnu konstrukciju kao karakter
- dobru prirodnu svetlost i pogled

Zato ne bih pravio "teski" rustik niti hladan minimalizam. Isao bih na:
- svetlu drvenu oblogu plafona u mat ulju
- ociscenu i prelakiranu opeku ili blago fugovanje, ne potpuno zatvaranje
- pod u srednje toplom hrastu ili kvalitetnom SPC/engineered oak tonu
- niske plakare pod obe kosine, dubina `45-60 cm`
- crna ili tamno bronzana rasveta po slemenu i na zabatima
- tekstil u toplim zemljanim tonovima: pesak, maslina, glina, siva lanena

## Predlog rasporeda
- Zona uz terasu i pogled: lounge + citaonica + mali radni sto
- Mirniji kraj uz dva prozora: spavaca zona
- Pod kosinama sa obe strane: neprekinuti niski plakari
- Oko stepenisnog otvora: lagana ograda od drveta i metala, ne puna zidna pregrada

## 7. Lokalni koncept renderi i skice

Napravio sam lokalne koncept-vizuale u folderu `renders/`. To nisu fotorealisticki renderi iz SketchUp/3ds Max merenog modela, nego namerno ciste koncept ilustracije bazirane na tvojoj osnovi i fotografijama, da mozemo brzo da zakljucamo pravac.

Fajlovi:
- `renders/contact-sheet.png`
- `renders/zoning-plan.png`
- `renders/render-1-warm-nordic.png`
- `renders/render-2-soft-japandi.png`
- `renders/render-3-rustic-studio.png`

## 8. Sta bih ja uradio prvo na terenu
1. proverio stanje folije i dasaka ispod crepa
2. izmerio stvarnu dubinu rogova i raster
3. proverio gde tacno moze da ide ventilacioni kanal
4. odlucio da li zadrzavas potpuno otvoren loft ili hoces pregradu za spavaci deo
5. tek onda zatvorio finalnu debljinu izolacije i tacnu nabavnu listu

## 9. Izvori
- Knauf roof insulation: https://www.knaufinsulation.com/what-we-do/our-solutions/mineral-wool-insulation-for-buildings/roof-insulation
- Pro Clima Intello: https://www2.proclima.com/products/internal-sealing/intello
- Roma NaturBoard FIT Plus: https://roma.rs/naturboard-fit-plus-knauf-4003010
- Knauf oficijelni NaturBoard FIT Plus data page: https://knauf.com/sq-XK/p/produkt/naturboard-fit-plus-23858_4217
- Roma izolacija krova i parne brane: https://roma.rs/izolacija-krova
- Crafter letva 3x5 3m: https://www.crafter.rs/letva-3x5-3m-090100302
- Krajina drvo lamperija: https://krajinadrvo.rs/proizvodi/brodski-pod-i-lamperija/lamperija/
- Aquaplan lamperija od finske omorike: https://www.aquaplanshop.rs/obloge-za-saune/lamperija-od-finske-omorike-14x95mm.html
- Daibau - pregled cena i smernice: https://www.daibau.rs/clanak/1857/izolacija_potkrovlja_-_stiropor_ili_mineralna_vuna
- Daibau - cenovni reperi po m2: https://www.daibau.rs/imenik/izolacija_potkrovja/trgoviste
- Svezaskele izolacija potkrovlja: https://www.svezaskele.rs/izolacija-potkrovlja/
